	HEALTH & SAFETY
Risk Assessment Form
	Assessment No.  RA-2026-018
Review date:  May 2027



	Company / Site
	Your Company — Main Warehouse
	Assessed by
	Facilities Manager
	Date
	November 4, 2026

	Activity / Area
	Loading dock and storage racking
	People at risk
	Staff, drivers, visitors
	Approved by
	



	#
	Hazard
	Who might be harmed & how
	Existing controls
	L
	S
	Risk
	Further action needed
	Owner
	Due

	1
	Forklift collision with pedestrians
	Staff and visitors — serious crush injuries
	Marked walkways; trained, licensed drivers
	3
	5
	15
	Install barriers at dock doors; add mirrors at blind corners
	Ops Mgr
	Dec 15

	2
	Falling stock from high racking
	Warehouse staff — head and body injuries
	Load limits posted; hard hats in racking aisles
	2
	4
	8
	Monthly racking inspection; anti-collapse mesh
	Facilities
	Jan 10

	3
	Manual handling of heavy boxes
	Pickers — back and shoulder strain
	Lifting training at induction
	3
	3
	9
	Provide trolleys; team lifts over 25 kg
	Supervisor
	Nov 30

	4
	Slips on wet floor near dock
	Anyone — sprains, fractures
	Wet-floor signs available
	3
	2
	6
	Anti-slip matting; spill kit at each dock
	Facilities
	Nov 20

	5
	
	
	
	
	
	
	
	
	

	6
	
	
	
	
	
	
	
	
	



	RISK MATRIX  (Risk = Likelihood × Severity)
	Likelihood ↓ / Severity →
	1
	2
	3
	4
	5

	5
	5
	10
	15
	20
	25

	4
	4
	8
	12
	16
	20

	3
	3
	6
	9
	12
	15

	2
	2
	4
	6
	8
	10

	1
	1
	2
	3
	4
	5



	KEY
■ 1–4  Low — manage with routine procedures
■ 5–9  Medium — action within 1 month
■ 10–14  High — action within 1 week
■ 15–25  Very high — stop work until controlled
Likelihood: 1 Rare • 2 Unlikely • 3 Possible • 4 Likely • 5 Almost certain
Severity: 1 Minor • 2 First aid • 3 Lost time • 4 Major injury • 5 Fatal

	

Assessor signature / date
	

Manager signature / date










